<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="1.143" y1="18.91245625" x2="1.143" y2="5.205778125" width="0" layer="20"/>
<wire x1="1.143" y1="5.205778125" x2="2.300778125" y2="3.54" width="0" layer="20" curve="90"/>
<wire x1="2.300778125" y1="3.54" x2="5.84076875" y2="3.54" width="0" layer="20"/>
<wire x1="5.84076875" y1="3.54" x2="6.554753125" y2="3.241878125" width="0" layer="20" curve="-45.32546"/>
<wire x1="6.554753125" y1="3.241878125" x2="9.369115625" y2="0.395353125" width="0" layer="20"/>
<wire x1="9.369115625" y1="0.395353125" x2="10.3159625" y2="0" width="0" layer="20" curve="45.325576"/>
<wire x1="10.3159625" y1="0" x2="118.8480375" y2="0" width="0" layer="20"/>
<wire x1="118.8480375" y1="0" x2="119.36" y2="0.5119625" width="0" layer="20" curve="90"/>
<wire x1="119.36" y1="0.5119625" x2="119.36" y2="22.540565625" width="0" layer="20"/>
<wire x1="119.36" y1="22.540565625" x2="118.11" y2="24.13" width="0" layer="20" curve="90"/>
<wire x1="118.11" y1="24.13" x2="10.87964375" y2="24.13" width="0" layer="20"/>
<wire x1="10.87964375" y1="24.13" x2="9.6394625" y2="23.63308125" width="0" layer="20" curve="43.670121"/>
<wire x1="9.6394625" y1="23.63308125" x2="6.72251875" y2="20.69519375" width="0" layer="20"/>
<wire x1="6.72251875" y1="20.69519375" x2="5.821284375" y2="20.32" width="0" layer="20" curve="-45.205105"/>
<wire x1="5.821284375" y1="20.32" x2="2.54" y2="20.32" width="0" layer="20"/>
<wire x1="2.54" y1="20.32" x2="1.143" y2="18.91245625" width="0" layer="20" curve="90"/>
<text>RED&gt;RED&gt;RED&gt;RED&gt;RED&gt;RED&gt;RED&gt;RED&gt;RED&gt;RED&gt;</text>
<text>+12v</text>
<text>+5v</text>
<text>-12v</text>
<text>MUSIC THING 
MODULAR
Power Stick 
125ma Max



Designed by 
Tom Whitwell
In Herne Hill, 
London. 


July 2015 
PCB Rev 1.1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dc-dc-converter">
<description>&lt;b&gt;DC-DC Converters&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="NMA">
<description>&lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="eurorack">
<packages>
<package name="POWER_16">
</package>
</packages>
</library>
<library name="thonkiconn">
<packages>
<package name="WQP-PJ301M-12_JACK">
</package>
</packages>
</library>
<library name="TomW">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="MusicThingModular">
<description>&lt;B&gt;Music Thing Modular parts library &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Components for Eurorack modular synths 
&lt;/ul&gt;</description>
<packages>
<package name="9MM_SNAP-IN_POT">
<description>9mm vertical snap-in pot, Alpha / Panasonic style</description>
</package>
<package name="7MM_RESISTOR">
<description>Standard resistor on 7mm grid</description>
</package>
</packages>
</library>
<library name="con-lumberg">
<description>&lt;b&gt;Lumberg Connectors&lt;/b&gt;&lt;p&gt;
include con-mfs.lbr - 2001.03.22&lt;br&gt;
Jack connectors - 2005.11.23&lt;p&gt;
http://www.lumberg.de&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1503_09">
<description>&lt;b&gt;Jack connectors according to JISC 6560, 3.5 mm&lt;/b&gt;&lt;p&gt;
Klinkeneinbaukupplung nach JISC 6560, 3,5 mm, 3-polig/&lt;br&gt;
stereo, abgewinkelte Ausführung, mit 2 Öffnern und Lötaugen,&lt;br&gt;
für Leiterplatten Rückseitenmontage&lt;p&gt;
Source: http://www.lumberg.com/Produkte/PDFs/1503_09.pdf</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="USB-A-H" value="USB-A-H"/>
<element name="DC1" library="dc-dc-converter" package="NMA" value="">
<attribute name="OC_NEWARK" value="61K3064"/>
<attribute name="MPN" value="NMA0515SC"/>
<attribute name="MF" value="C &amp; D TECHNOLOGIES, INC"/>
<attribute name="OC_FARNELL" value="1021434"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="eurorack" package="POWER_16" value="POWER"/>
<element name="J1" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK"/>
<element name="VR1" library="MusicThingModular" package="9MM_SNAP-IN_POT" value="50K B"/>
<element name="X1" library="con-lumberg" package="1503_09" value="1503_09">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1243244"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="MusicThingModular" package="7MM_RESISTOR" value="2k"/>
<element name="R2" library="MusicThingModular" package="7MM_RESISTOR" value="2k"/>
<element name="R3" library="MusicThingModular" package="7MM_RESISTOR" value="2k"/>
<element name="+12" library="TomW" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="-12" library="TomW" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="5V" library="TomW" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="gm-caps-electro-pol" package="050_020" value="47uf 16v">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="eurorack" package="POWER_16" value="POWER"/>
<element name="U$3" library="eurorack" package="POWER_16" value="POWER"/>
<element name="U$4" library="eurorack" package="POWER_16" value="POWER"/>
</elements>
<signals>
<signal name="5V">
<contactref element="DC1" pad="1"/>
<contactref element="U$1" pad="11"/>
<contactref element="U$1" pad="12"/>
<contactref element="JP1" pad="VBUS"/>
<contactref element="C1" pad="+"/>
<contactref element="U$2" pad="11"/>
<contactref element="U$2" pad="12"/>
<contactref element="U$3" pad="11"/>
<contactref element="U$3" pad="12"/>
<contactref element="U$4" pad="11"/>
<contactref element="U$4" pad="12"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="DC1" pad="6"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="10"/>
<contactref element="U$2" pad="9"/>
<contactref element="U$2" pad="10"/>
<contactref element="U$3" pad="9"/>
<contactref element="U$3" pad="10"/>
<contactref element="U$4" pad="9"/>
<contactref element="U$4" pad="10"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="-12V">
<contactref element="DC1" pad="4"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$4" pad="2"/>
<contactref element="U$4" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="P$1"/>
<contactref element="VR1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="VR1" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="COM">
<contactref element="DC1" pad="5"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="8"/>
<contactref element="J1" pad="P$3"/>
<contactref element="VR1" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="DC1" pad="2"/>
<contactref element="JP1" pad="GND"/>
<contactref element="C1" pad="-"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="7"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$3" pad="7"/>
<contactref element="U$3" pad="5"/>
<contactref element="U$3" pad="6"/>
<contactref element="U$3" pad="8"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$4" pad="7"/>
<contactref element="U$4" pad="5"/>
<contactref element="U$4" pad="6"/>
<contactref element="U$4" pad="8"/>
<contactref element="U$4" pad="4"/>
<contactref element="5V" pad="K"/>
<contactref element="+12" pad="K"/>
<contactref element="-12" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="13"/>
<contactref element="U$2" pad="14"/>
<contactref element="U$2" pad="13"/>
<contactref element="U$3" pad="14"/>
<contactref element="U$3" pad="13"/>
<contactref element="U$4" pad="14"/>
<contactref element="U$4" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$2" pad="16"/>
<contactref element="U$2" pad="15"/>
<contactref element="U$3" pad="16"/>
<contactref element="U$3" pad="15"/>
<contactref element="U$4" pad="16"/>
<contactref element="U$4" pad="15"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="5V" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="+12" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="-12" pad="K"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
